|  |  |
| --- | --- |
| The **C501** electronic thermostat features a floor temperature sensor and is designed for wall mounting in a standard recessed box. It includes a 3-meter floor temperature sensor cable for convenient installation. | \\dc\temp\MARKETINGAS\Comfort Heat_WEB\CH_MediaPark\Produktai web\Foto_apdirbtos_web\C501\501_Jussi.png |

**TECHNICAL DATA**

|  |  |
| --- | --- |
| Voltage | 230V AC 50/60 Hz |
| Max load | 14 A / 3200 W |
| ON / OFF switch | Built-in interrupter 1-pole |
| Temperature range | +5°C ... +40°C |
| Hysteresis | +/-0,4°C |
| Setting of the temperature range | Min / max |
| Sensor type | Floor (NTC) |
| Sensor resistance | 14,8 kOhm / 20°C |
| Temperature setback | fixed 5°C |
| Light indicator | LED |
| Dimensions | 80x80x50 mm |
| Protection class | IP21 |
| Warranty | 3 year |

**PRODUCT LIST**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Type** | **Temperature range** | **Sensor** | **Model** | **Stock code** |
| C 501 | +5°C ... +40°C | Floor, 3 m | Jussi | 19115952 |

**WIRING DIAGRAM**

|  |  |
| --- | --- |
| **\\dc\temp\MARKETINGAS\Comfort Heat_WEB\CH_MediaPark\Produktai web\Foto_apdirbtos_web\C501\C501 scheme.jpg** |  |