|  |  |
| --- | --- |
| The electronic clock thermostat **Comfort Touch**, with a fine LCD display, comes with a floor temperature sensor and energy consumption management system.  **Comfort Touch** thermostat has pre-programmed functions adjusted to Lithuanian climate and weekly mode. Factory settings and data are retrieved beyond power failure.  The thermostat is wall-mounted into a standard recessed box. The energy consumption management system informs of the percentage consumption of adjusted temperature levels, what your monthly consumption is, and the upcoming year’s expenditure. |  |

**TECHNICAL DATA**

|  |  |
| --- | --- |
| Voltage | 100-230 V AC 50/60 Hz |
| Max load | 16 A / 3600 W |
| Screen | 2”, 176x220 points, touchscreen |
| ON / OFF switch | Built-in interrupter 2-pole |
| Standby mode energy consumption | < 0,5 W |
| Temperature range | +5°C ... +40°C |
| Hysteresis | 0,4°C |
| Energy consumption and saved time memory | 5 year |
| Saved programming | Unlimited time |
| Sensor type | Floor (NTC) and room |
| Sensor resistance | 14,8 kOhm / 20°C |
| Dimensions | 84x84x40 mm |
| Protection class | IP21 |
| Warranty | 3 year |

**PRODUCT LIST**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Type** | **Temperature range** | **Sensor** | **Model** | **Stock code** |
| Comfort Touch White | +5°C ... +40°C | Floor and room, 3m | Elko | 19115967 |
| Comfort Touch Black | +5°C ... +40°C | Floor and room, 3m | Elko | 19115968 |

**WIRING DIAGRAM**

|  |  |
| --- | --- |
|  |  |